**Business name: The Australian Wine company**

Method of water treatment: Rainwater is treated with UV filter

What is monitored/checked to ensure treatment is effective (e.g. pH, freely available chlorine)? Full chemical analysis of water; and UV filter is serviced monthly and replaced annually.

Frequency of monitoring: Quarterly

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Date/time** | **Result** | **Is water treatment effective?** (Yes/No) | **If no, detail the action taken** | **Checked by** |
| 30/3/21 | All good | Yes | No action required – refer to chem analysis results for AWQC | G. Darling |
| 30/6/21 | All good | Yes | No action required – refer to chem analysis results for AWQC | G. Darling |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |